{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":16,"n_cols":13,"rows_kept":16,"cut":false,"hidden":false,"merged":[[9,7,10,7],[9,9,10,9],[0,0,0,12],[8,1,11,1],[12,7,12,9],[2,4,15,4],[2,5,15,5]]}
["自动水位雨量监测站报价"]
["设备名称         供应商名称","武汉新普惠（元）\n（报价含运费含税）","型 号","备 注","深圳市佳佳眼科技（元）\n（含税报价，不含运费不含安装）","型号","备注","上海晶奕测控（元）\n（含税报价，不含运费）","型 号","备注","深圳南方安创\n（含税报价，不包运费）","型 号","备注"]
["立杆",3600,"PH-3","含水位横臂",28800,"无","4米",1411,"CP-UPP-EQ101/35","3.5m立杆",4200,"立杆3.5米+摇臂3米+太阳能板架"]
["机箱",1050,"PH-FHX",{"$nulls":4},6316,"CP-STB-STD1V",null,450,"不锈钢含抱箍400*500"]
["RTU（含4G模块）",6600,"PH-282",{"$nulls":4},"/","/","包含在机箱",2400,"/"]
["翻斗式雨量计",2040,"PHYL",{"$nulls":4},1276,"CP-RN301",null,6600,"/"]
["雷达水位计",10200,"PH-LDYW",null,null,null,"量程20米",4670,"CP-BYE130","10米量程",15600,"雷达30米量程"]
["信号避雷器",600,"PH-FL",{"$nulls":4},1008,"CP-BYE-EK10K","双模式避雷解决方案\n外置避雷氧化锌放电管+地线方式配合机箱中内置的避雷装置，与外置避雷装置共同发生作用，确保安全可靠。",540,"/"]
["太阳能板",3600,"定制",null,null,null,"100W",504,"CP-SRP-EQ20W",null,1350,"单晶130W"]
["充电保护器",null,"定制",{"$nulls":4},"/","/","机箱内含",240,"/"]
["蓄电池（免维护）",null,"英菲凌",{"$nulls":5},"/",null,2520,"80AH高效锂电池"]
["接插件及信号线缆",null,"定制",{"$nulls":4},739,"/","杆内置接线插头及引线，现场直接接插式安装",360,"/"]
["基础",6000,"定制",{"$nulls":4},"当地提供，根据贵阳行情预估1200",null,null,300,"地笼"]
["安装调试及接入费用",9000,"新普惠定制",{"$nulls":4},"/","/","“免培训型”安装，安装工人插接即可，发货前调好参数，无须现场调试。","/","免费技术支持"]
["SIM卡",300,"移动","3年流量费",null,null,null,403,"/","每台设备接入仅需10元，无其它费用，可续费",300,"/"]
["合计：",{"$f":"SUM(B3:B15)","v":42990},{"$nulls":5},{"$f":"SUM(H3:H15)","v":16327},null,"本方案使用标准版机箱，机箱质保2年，传感器质保1年，3年成本费维修。（企业版报价3万多）",{"$f":"SUM(K3:K15)","v":34860}]